Empowered by Innovation

# NEC MultiSync® E223W

Order Code: 60003334 (bk), 60003335 (wh) NEC LCD 22" Commercial Display

NEC MultiSync E223W features an extremely thin LED backlight panel which results in an ultra-modern and slim design in combination with a perfect feature set for the standard corporate office. The display offers 110 mm height adjustment and a broad connectivity wiht three inputs DisplayPort, DVI-D and D-Sub.

Ideal for the corporate that demand style and future proof technology.

**DELIVERING GENUINE BENEFITS**

Image display - 22inch 16:10 TN with LED backlight.

Ergonomic Office - full height adjustability (110 mm), swivel, tilt and pivot functionality ensures perfect individual ergonomic set-up.

Vesa Mount (100 mm) - allows to install the monitor via various mounting solutions.

Free Download of Multi-Display Management Software - with NaViSet Administrator 2 you can manage all your connected display devices from a centralized location.



Administrator 2

**OUTSTANDING PERFORMANCE**

. Ultra-modern and slim design. The product design is discrete and puts priority on the screen image and function.

. Excellent ergonomics. The ergonomic stand with 110 mm height adjustability allows greatest set-up flexibility.

. Low energy consumption with LED backlight and unique Carbon Savings Meter.

This document is © copyright 2014 NEC Display Solutions Europe GmbH.

All rights reserved in favour of their respective owners. All hardware and software names are brand names and/or registered trademarks of the respective manufacturers. All specifications are subject to change without notice. Errors and omissions are excepted. 24.02.2014

[www.nec-display-solutions.com](http://www.nec-display-solutions.com)

**NEC MultiSync® E223W**

**SPECIAL CHARACTERISTICS**



|  |  |
| --- | --- |
| Technical Specification NEC MultiSync® E223W | |
| DISPLAY |  |
| Panel Technology | W-LED TN TFT |
| Screen Size [inch/cm] | 22 / 55.87 |
| Screen Aspect Ratio | 16:10 |
| Pixel Pitch [mm] | 0.282 |
| Brightness (typ.) [cd/m2] | 250 |
| Contrast Ratio (typ.) | 1000:1 (25000:1 dynamic contrast ratio) |
| Viewing Angle [°] | 170 horizontal / 160 vertical (typ. at contrast ratio 10:1); 178 horizontal / 178 vertical (typ. at contrast ratio 5:1) |
| Response Time (typ.) [ms] | 5 |
| Colours [Mio.] | 16.7 |
| SYNCHRONISATION RATE |  |
| Horizontal Frequency [kHz] | 31.5 - 82.3 |
| Vertical Frequency [Hz] | 56 - 75 |
| RESOLUTION |  |
| Optimum Resolution | 1680 x 1050 at 60 Hz |
| Supported | 1680 x 1050; 1600 x 1200; 1440 x 900; 1400 x 1050; 1366 x 768; 1360 x 768; 1280 x 1024; 1280 x 960; 1280 x 768; 1280 x 720; 1024 x 768; 800 x 600; 640 x 480 |
| CONNECTIVITY |  |
| Digital | 1 x DVI-D (with HDCP); 1 x DisplayPort |
| Analog | 1 x mini D-sub 15 pin |
| ELECTRICAL |  |
| Power Consumption on Mode [W] | 17 (typ.); 12 (Eco Mode); 24 (max.) |
| Power Savings Mode [W] | 0.35 |
| Power Supply | 100-120 V/220-240 V; 1 A/0.5 A; integrated power supply |
| ENVIRONMENTAL CONDITIONS |  |
| Operating Temperature [°C] | +5 to +35 |
| Operating Humidity [%] | 20 to 80 |
| ERGONOMICS |  |
| Height adjustable stand [mm] | 110 |
| Screen Tilt / Swivel [°] | -5 to +20; -45 to +45 |
| Screen Rotate [°] | 0 to 90 (landscape to portrait mode) |
| MECHANICAL |  |
| Bezel Width [mm] | 13.9 (left and right); 15.8 (top and bottom) |
| Dimensions (W x H x D) [mm] | 503.5 x 383.3 x 213.9 |
| Weight [kg] | 5.6 |
| VESA Mounting [mm] | 100x 100 |
| ADDITIONAL FEATURES |  |
| Colour Versions | White Front Bezel, White Back Cabinet; Black Front Bezel, Black Back Cabinet |
| Cable Management | yes |
| Kensington security slot | yes |
| Plug and Play | VESA DDC/CI; DDC2B/2Bi |
| Adjust Functions | Auto Adjust; Brightness; Colour Temperature Control; Contrast; DV Mode; EcoMode; Fine Adjust (analog); Intelligent Power Management; Language Select; LED Brightness; Monitor Information; NTAA (Non-Touch-Auto-Adjustment); OnScreen-Display (OSD) lock-out; Power-Off Timer; sRGB |
| Shipping Content | Monitor; Power Cable; CD-ROM; Sales Office List; User Manual Signal Cable: VGA - VGA; DVI-D - DVI-D |
| Safety and Ergonomics | EPEAT Silver™; EPEAT™ Gold (black version); CE; ErP; TCO 6.0; TUV Ergonomics; TUV GS; GEEA/Energy Label; Energy Star 5.0; FCC Class B; PCT/Gost; UL/C-UL or CSA; ISO 9241-307 (pixel failure class I); MPR II/ MPR III; RoHS |
| Warranty | 3 years warranty incl. backlight |

Energy Efficiency Carbon Footprint Meter / Carbon Savings Meter; ECOMode; Intelligent Power Management; LED backlight technology

|  |  |
| --- | --- |
| Ecological Materials | Downloadable manuals |
| Ecological Standards | TCO 5.2 |

Carbon Footprint Meter, Carbon Savings Meter, EcoModes, ErgoDesign®: Height adjustable stand (110 mm) with 90° Pivot features, NaViSet Administrator 2, sRGB Support, Touch Sensor Keys, WindowsVistaCertifiedLogo



Empowered by Innovation